{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":37,"n_cols":3,"rows_kept":37,"merged":[[1,0,1,2],[9,0,11,0],[14,0,15,0]],"flags":["formulas_cached_only"]}
["附件2"]
["门店组装设备采购清单"]
["①店铺主体结构制作"]
["项目","材质/规格","数量"]
["设计制作（含场地勘测）","符合98平米空间布局，含图纸设计","1套"]
["店铺主体结构制作","6MX11.4M，箱顶聚氨酯双面铝板保温隔热，外墙铝钢板，内部100*100mm方钢龙骨做主体，填充聚氨酯保温隔热层，\n安装到位，表面喷漆，整体防水防腐处理，内部结构按需制作","1套"]
["顶棚瓦面","成品瓦片","69平方米"]
["②基础装修"]
["项目","材质/规格","数量"]
["地面处理","地面填平:斜坡高差约30厘米不平整\n1.原有地面石材剔除12m，宽7m。\n2.红砖砌一个12m×7m的长方形24cm宽平均水平高度20cm高的围挡。\n3.用石粉回填12m乘7m平均深度回填在20cm的回填层。\n4.人工河沙水泥找12m×7m厚度5cm的地面找平层。","/"]
[null,"找平层、铺贴800mmX800mm防滑耐磨亚光地砖","53平方米"]
[null,"找平层、铺贴300mmX300mm防滑耐磨亚光地砖","16平方米"]
["墙面处理","集成墙板","80平方米"]
["天花板处理","吊顶安装，含堂食区灯具预留孔35个，储物间3个","69平方米"]
["门窗安装","地弹玻璃门:12mm厚钢化1400X3000mm玻璃双开门，正面2扇，背面1扇","3套"]
[null,"玻璃幕墙:12mm厚钢化玻璃墙正面正面3块(1850X3000+5350X3000+3698X300)mm、背面背面2块（1950X3000+1752X3000）mm","42平方米"]
["水电安装","线路铺设，管道铺设，含开关插座等","1套"]
["③就餐区与服务区"]
["项目","材质/规格","数量"]
["桌椅配置","8张方形桌子，26把椅子，3个长条卡座","1套"]
["收银台与吧台","红砖墙体基础台面钢结构龙骨及木工板基础石材台面","1套"]
["展示柜","IP形象雕塑1个，双面实木展示柜1套，装饰若干","1项"]
["装饰与绿植","墙面装饰画2套、店内绿植","1项"]
["④照明与空气管理"]
["项目","材质/规格","数量"]
["照明设备","室内LED灯38个、室外射灯12个","1套"]
["空气管理","吊装及排气系统","1套"]
[null,"制冷系统","1套"]
["⑤安全与卫生设施"]
["项目","材质/规格","数量"]
["消防系统","灭火器、烟雾报警器、应急指示标识等","1套"]
["洗手池设施","陶瓷洗手池","1套"]
["⑥杂项与预留"]
["项目","说明"]
["户外外摆区","花箱","10个"]
["户外外摆区","户外座椅板凳","4套"]
["材料运输","运输费用及清洁保洁"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}