{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["新"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"新","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"merged":[[1,1,1,5]]}
[null,"附件3"]
[null,"经营设备清单"]
[null,"序号","品名","规格参数明细","数量","备注"]
[null,1,"收银系统全套","\n显示屏15.6英寸 1366x768分辨率\n四核CPU 大容量存储16GB\n内存2GB\nAndroid系统操作系统\n含收银软件",1]
[null,2,"监控系统","室内半球：\n默认2.8mm广角镜头，可视角度100度；\n室外枪机：\n默认4mm星光镜头，可视角度85度；\n可混搭使用。",5]
[null,3,"厨房油烟净化器","电源；220V-HZ\n主电机输入功率；1200w\n风量；32m³/min\n照明功率；S3W\n静压值；380Pa\n整机尺寸(宽x深x高)；1200*800*500mm\n净化器尺寸；300*400*320mm\n烟管直径；200mm",1]
[null,4,"立式四门全冷冻冰箱","尺寸:1200mmX740mmx1970mm\n重量:123kg\n容量:1000L\n功率:240~300W\n温度范围:-5°C≤-15°C",1]
[null,5,"吧台式冷藏柜1","尺寸1500mm*700mm*800mm\n1台需台面挖槽6个放置小冰桶\n功率：395w\n温度：（2-8）°C\n冷凝方式：冷藏",1]
[null,6,"吧台式冷藏柜2","尺寸：1200mm*700mm*800mm\n功率：380w\n温度：（2-8）°C\n冷凝方式：冷藏",1]
[null,7,"吧台式制冰机带冰铲","产冰量100kg \n储冰量：40kg\n电压、功率 ：220V/500W\n冰型：方型\n制冷方式：水冷制冷\n机器尺寸mm:700*700*800",1]
[null,8,"不锈钢双水槽\n含龙头水管","整体尺寸（mm）：1000*700\n水槽单个尺寸（mm）：400*400/个",1]
[null,9,"挂式净水器","超滤机，中央净水机\n工作原理：超滤\n功效：直饮\n额定出水量：1000L/h\n滤芯：中空纤维，PP棉，活性炭纤维，\nPPF棉，活性炭+超滤，超滤膜",1]
[null,10,"挂式开水机","内胆材质304不锈钢\n两用冷热挂壁式开水器商用步进式\n显示屏类LCD型\n加热方式步进式\n净重；12kg  最大容积；60L\n功率；3KW  额定出水；60L/h",1]
[null,11,"不锈钢保温小冰桶","直径约10cm,304不锈钢材质，",10]
[null,12,"煮面桶","60型电热U形管\n容积170L 电热攻略12KW\n电压220/380V 内外直径60/65cm\n外高度85cm 滤网深度40cm 尺寸 65X65X85",1]
[null,13,"暴打套装","常规套装",1]
[null,14,"自动加热调料台","尺寸：约70cmX57cm\n电压：220V\n30-110°温度调节",1]
[null,15,"电炸锅","EF-101V电炸炉\n产品容量10L\n产品重量6kg\n外形尺寸280x460x305mm\n油缸尺寸265x328x150mm\n炸网尺寸200x210x110mm\n温控范围60-200°C\n产品电压220V/50Hz\n产品功率3kW",1]
[null,16,"电蒸保温箱","名称；五层铝架蒸包柜\n型号；ASQ-500\n尺寸；380x400x745mm\n电压；220V\n功率；1200W\n容量；50-60个\n层架间距；80mm\n层架尺寸；300x300mm\n温控范围；30-110℃",1]
[null,17,"封口机","机器尺寸：250*395*620mm\n型号；BST-FKJ01\n功率；280W",1]
[null,18,"多功能分杯架","常规款",1]
[null,19,"烤肠机","\n型号；008-2\n电压；220V\n",1]
[null,20,"果糖机","功能；智能提醒\n颜色分类；白色\n尺寸；260*250*401\n功率；360\n容量；8L",1]
[null,21,"不锈钢置物架","尺寸（mm）：850*300*800\n颜色分类；银白色",1]
[null,22,"不锈钢水槽","尺寸（mm）（外600*600 内400*400）",1]
[null,23,"电磁炉","型号YFR-QN3502A\n灶眼数量单个\n灶面类型凹面灶\n最大承重100kg(含)-300kg(不含)\n功率\n3500W 4200W 5000W",1]
[null,24,"微波炉","容量 20L(含)-25L(含)\n功率 600W(含)-900W(含)\n能效等级 1级",1]
[null,25,"收银出餐操作台面柜","2400mmx700mmx800不锈钢操作台面柜\n下方设置3个隔断储物柜",1]
[null,26,"厨房油水分离器","500mmX290mmX290mm\n厨房不锈钢排水商用过滤器",1]